# ADDENDUM #1

1. **Deletions**
2. Remove ALL Type 3 Removals.
3. Remove BR Location #636, boiler-surface parging cement.
4. **Clarifications**
5. The new duct liner, specified in ‘Appendix A: Project #5’ is to be laid on the existing linear ceiling. It replaces the existing duct insulation liner which is deteriorating.
6. There will be a separate tender for Type 3 Removals, which will be a revised list.