**All Projects:**

Ceiling paint: #03360, by Cloverdale

Wall paint: #OW134, “It’s a Cream”, by Cloverdale

Wall gypsum board: ½” thick

Ceiling gypsum board: Type X, 5/8”

Fireproofing ‘*blue*’ paint: #7408 “Sunrise River”, by Cloverdale

Ceiling Tile: CGC: DX/DXL 15/16” Acoustical Suspension System.

**Project No.1** Residence (Bartley & Prettie)

Prettie and Bartley Residences: remove listed mechanical asbestos items; and replace with ‘like’, non-asbestos material, unless otherwise indicated.

**Project No. 2:** Main campus: Miscellaneous

Greenhouse (GH), Univeristy Centre (UC), and Sanders Fieldhouse (SB).Remove listed asbestos and replace with ‘like’, non-asbestos materials.

**Project No. 3:** Mechanical asbestos items

Power House (PH), Sanders Fieldhouse (SB), School of Nursing (SN), Centennial Building (CB), Bora Laskin (BL), Library (LI), Avila Centre (AC), Braun Building (BB), University Centre (UC), and Ryan Building (RB).

**Project No. 4:** Type 3 Removals

Remove asbestos fireproofing, (and linear ceiling where applicable) in Centennial Building, University Centre, and Ryan Building, all various locations. Replace with cementicious fireproofing, painted blue, new Toughgard T Textile Duct Liner, by CertainTeed laid on new suspended ceiling by CGC: DX/DXL 15/16” Acoustical Suspension System and flush mount: standard LED tube fixture, (where applicable). Patch and paint where required.

**Project No. 5:** Type 2 Cleaning

Remove linear ceiling and asbestos fireproofing in ceiling space. Replace existing black paper with new Toughgard T Textile Duct Liner and put back cleaned, existing linear ceiling.